**Technical Specification**

**Contact Address:** The Carnegie Theatre

Finkle Street

Workington

Cumbria

CA14 2BD

**Telephone No's:** All Departments 01900 602122

**Email:** technical@carnegietheatre.co.uk

Karen Thompson Theatre Manager

Nigel Roebuck Technical Manager

Daniel Marsden Box Office & Admin Manager

**Capacity:**

Seated: 306 Stalls: 184 Balcony: 122

**SAT NAV:**

Users should enter our postcode CA14 2BD

For Get in and stage use CA14 2BN

**Get-in:**

The Theatre is situated on ground floor of the building. Dock doors 1.5m x 3m. Postcode CA14 2BN.

**The following stock list is by no means our full stock but represents the most commonly asked for equipment in our inventory.**

**If you need something that isn’t listed please get in touch with our technical department and we will do our best to assist you.**

**Stage Area:**

Wooden Raked Proscenium Arch Stage

Load in point: Dock Doors to rear of stage

Performing Area: 9m x 8m

Pros opening: 7m x 6m.

Forestage: 3m x 1m

Wing Widths: 2m SR, 2m SL.

Sprung Floor

Grid: 5.0m

No fly tower

2 tab tracks

Red House Tabs operated from stage right

Orchestra Pit: 7m x 2m suitable for up to 15 (This is normally covered to provide a 2m thrust but the cover can be removed by prior arrangement. A fee may be charged for this. please enquire)

Cross Over: Across back of stage

Legs: Yes Black

Borders: Yes Black

Back Cloth: Black Fibre optic star cloth or white cyclorama

**Backstage:**

5 dressing rooms – access from stage & balcony

1 x Shower

Green Room

Adequate supply of power points

Catering available

Rehearsal Rooms

Stage, Backstage & Dressing Room facilities not accessible to mobility impaired performers & staff

**Stage Power:**

1 x 63a 3 phase supply on Ceeform socket.

Our internal dimmer power feeds can be switched to:-

1 x 63A 3 phase supply and 1x 32A 3 Phase supply both on Ceeform Sockets.

To facilitate connection of touring rigs.

**All electrical equipment brought onto the premises MUST carry a current Portable Appliance Test ( PAT) certificate, otherwise its use may not be permitted.**

**Lighting:**

ETC Ion Lighting Desk with 40ch Fader Wing 2 universes 1024 addresses operated from rear stalls.

In addition, a spare DMX line for touring rigs is available

ETC Nomad with 2 universes of DMX on Running on MACBook Pro

48 Channels of ETC Colour source dimming

4 x Chauvet Qspot 560 led Moving Head spots

4 x Chauvet Qwash 436z led Moving Head Wash

4 x Chauvet Colouredash Par quad 18 led wash lights

12 x Selicon Pacific Zoom Spots all in FOH Bridge

4 x ETC Source 4 Juniors

48 x par64 1000w fitted with a mix of CP61 and 62 lamps

16 x Fresnel’s 1000w

8 x Rank Strand Coda 1000w floods

4 x Rank Strand Coda 3 way 500w Cyc Battens

2 x Rank Strand 2000w follow spots operated from Rear Balcony

**Fx:**

1 x Le Maitre Neutron Hazer with DMX Control

A DMX patch and channel list is available on request.

**Sound:**

**Desks**

1 x Yamaha LS9-32 Digital mixer

1 x Allan and Heath 16ch Mix wizard

1 x Mackie 1642-VLZ3 16ch

**Multicores**

1 x Klotz 32/4 Multi Fixed in Main House

1 x 24/8 Multi Fixed in Monroe’s Bar

1 x Peavy 16/4 Multi

1 x Peavy 12/4 Multi

**Loudspeakers**

4 x Yamaha DSR118W 800w powered sub bass

2 x Yamaha DSR215 1300W Class D Biamped box

4 x Yamaha DSR112 300W

4 x ElectroVoice SRX 100

**Microphones**

2 x Shure SM58

4 x Shure SM58 BETA

3 x Shure SM57

2 x Shure PG52

3 x Shure PG56

2 x Shure PG81

5 x Orchid Electronics active DI Box

Large selection of audio cabling available

8 K & M Boom Mic Stand Black

4 K & M Small table mic stand

5 K&M Drum Clip

Acoustics suitable for music & spoken word

**Please contact the technical department if you need something that’s not on the list as we are adding to stocks continually.**